Abstract Robot Control Language (ARCL)

This is the intermediate language used for SCARL. This language is structed as to be suitable to be converted to either assembler or to code that is used for robotics control. The abstract machine is one that utilizes ports and has a simple memory layout. We define the instruction set for the Abstract Robot here and provide the instruction’s close relative within the Atmel AVR Instruction Set.

Important in this language is the flags for the SCARL linker that says to generate code for a specific device action. It is up to the SCARL linker (it will be a compiler-linker combination) to perform the final conversion when it runs into such a directive, as the implementation of the device may vary from machine to machine.

Description of the abstract machine that ARCL runs on:

A machine that:

1. Has a 8 general purpose 16 bit registers.
2. Has a special implicit frame pointer register
3. Special register for returning function values called “FRR”
4. Has a stack with unbounded memory
5. Has a space of read-only memory that is set before execution of the program.
6. Each atomic object is a 2 byte word that can be interpreted in multiple different ways
7. Has a set of peripheral pins that may be set to input or output, and have power on, or read the power from it

Instruction Set Table

|  |  |
| --- | --- |
| **Expression Instructions** | **Action** |
| ADD *reg1 reg2* | Add the two registers, storing the result in the right hand side register |
| SUB *reg1 reg2* | Subtract the two registers *reg1 – reg2*, storing the result in the right hand side register |
| MULT *reg1 reg2* | Multiply the two registers, storing the result in the right hand side register |
| DIV *reg1 reg2* | Integer division on the two registers *reg1 / reg2*, storing the result in the right hand side register |

|  |  |
| --- | --- |
| **Memory Instructions** | **Action** |
| MOV *src dst* | Moves data from the *src* register to the *dst* register |
| LOADL *reg lit* | Loads the register *reg* with the literal *lit* |
| LOADF *reg offset* | Loads the value stored *offset* values away from the top of the stack frame and loads it into register *reg* |
| LOADR *reg offset* | Finds the value from static storage that is *offset* values away from the beginning of static storage and stores it into register *reg* |
| STORF *reg offset* | Goes to the value located *offset* values away from the top of the stack frame and changes it so that it is equal to the value located in the register *reg* |
| STORR *reg offset* | Loads the value in register *reg* into the spot that is *offset* values away from the beginning of static storage. |
| FRAMEU *offset* | Push the stack frame so that it is *offset* values farther away. For setting up actvation record space |
| FRAMEO *offset* | Pop the stack frame so that it is *offset* values closer. For removing activation record space |

|  |  |
| --- | --- |
| **Program Control Instructions** | **Action** |
| LABEL *label* | Defines a label at this spot and calls it *label* |
| PROC *label* | Begins a procedure definition and calls it *label* |
| RET | Returns control back to the callee from a procedure call |
| CALL *label* | Creates an activation record for the procedure called *label* and transfers program execution to that procedure |
| JMP *label* | Jumps to the label *label* |
| CMP *reg1 reg2* | Compares the two registers *reg1* and *reg2* and changes the internal state of this ARCL machine. (see below) |
| JPE *label* | Jump to the *label* if the most recent CMP had *reg1 == reg2* |
| JPNE *label* | Jump to *label* if the most recent CMP had *reg1* != *reg2* |
| JPGR *label* | Jump to the *label* if the most recent CMP had *reg1* > *reg2* |
| JPLS *label* | Jump to the *label* if the most recent CMP had *reg1 < reg2* |
| JPGE *label* | Jump to the *label* if the most recent CMP had *reg1* >= *reg2* |
| JPLE *label* | Jump to the *label* if the most recent CMP had *reg1 <= reg2* |
| JAND *label* | Jump to *label* if the most recent CMP evaluates to true under the following conditions:   |  |  |  | | --- | --- | --- | | *reg1* | *reg2* | evaluation | | not 0 | not 0 | true | | 0 | not 0 | false | | not 0 | 0 | false | | 0 | 0 | false | |
| JOR *label* | Jump to *label* if the most recent CMP evaluates to true under the following conditions:   |  |  |  | | --- | --- | --- | | *reg1* | *reg2* | evaluation | | not 0 | not 0 | true | | 0 | not 0 | true | | not 0 | 0 | true | | 0 | 0 | false | |

|  |  |
| --- | --- |
| **Device Control Instructions** | **Action** |
|  |  |
|  |  |
|  |  |
|  |  |